Product description

|  |  |
| --- | --- |
| Dimensions | https://onlineshop.ms-motorservice.com/msi/html/page/help.png |
| Type | exhaust valve |
| Packing unit | 2 |
| Valve head diameter (D) | 35.4 mm |
| Skirt diameter (d) | 8.0 mm |
| Length (L) | 124.7 mm |
| Valve seat angle (α) | 45° |
| Valve stem treatment | chromium-plated (Cr) |
| Skirt end treatment | hardened |
| Material 1 | Bimetallic version (A/S) |
| Reference numbers | 0428 0049 |