Product description

|  |  |
| --- | --- |
| Dimensions | https://onlineshop.ms-motorservice.com/msi/html/page/help.png |
| Cylinder diameter (Ø) | 91.0 mm |
| Compression height (KH) | 55.17 mm |
| Bowl depth (MT) | 19.81 mm |
| Bowl diameter (MØ) | 40.0 mm |
| Total length (GL) | 86.27 mm |
| Pin diameter (BoØ) | 26.0 mm |
| Pin length | 65.0 mm |
| Casting number | 091 034 |
| Piston rings 1, 2, 3   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | 1 | × | R | 2 mm | CR | G6 | | 1 | × | M | 2 mm |  |  | | 1 | × | DSF | 3 mm |  |  | | |