Product description

|  |  |
| --- | --- |
| Dry cylinder liner | |
| Machining condition | finished |
| Dimensions | https://onlineshop.ms-motorservice.com/msi/html/page/help.png |
| Cylinder diameter (D) | 94.0 mm |
| Register diameter (A) | 98.5 mm |
| Flange diameter (C) | 102.5 mm |
| Installation height (H) | 5.0 mm |
| Total length (L) | 196.0 mm |